        #
        | README file for
        |
        | ELSA Windows 95/98 Driver Disk, ver 4.10.01.0303-0004
        |
        |       VICTORY Erazor AGP/ PCI
        |
        | Copyright (c) 1994-98 ELSA AG, Aachen (Germany)
        |
        | ELSA AG                    Internet   : http://www.elsa.de
        | Sonnenweg 11               LocalWeb   : +49-(0)241-938800
        | D-52070 Aachen             
        |
        | ELSA Inc.                  Internet   : http://www.elsa.com
        | 2231 Calle De Luna         
        | Santa Clara, CA 95054
        | USA
        |
        | ELSA Asia Inc.             Internet   : http://www.elsa.com
        | 7F-11, No. 188, Sec. 5     
        | Nanking East Road
        | Taipei 105
        | Taiwan, R. O. C.
        |
        | ELSA Japan Inc.            Internet   : http://www.elsa.com
        | Mita Suzuki Building 3F                
        | 5-20-14 Shiba, Minato-ku
        | Tokyo 108-0014
        | Japan
        |
        | 08/11/98, MWolf


        Contents

        1. Overview
        2. Contents
        3. Installation
        4. History
        5. Release Notes
        6. Known Bugs and Operating Notes


------------------------------------------------------------------------

1.      Overview

        This CD contains the ELSA Display Driver for Microsoft Windows 95/98.

        The driver supports 256, 65536 and 16 Million colors in
        all resolutions available on used ELSA board.

        NOTE:

        It is not possible to use a TV and a computer monitor at the same
        time!

------------------------------------------------------------------------

2.      Contents

        This directory contains the following files:

        README.TXT      the file you currently look at
        LIESMICH.TXT    german version of README
        ELSAVEAD.DRV    display driver file for VICTORY Erazor
        ELSAVEAX.DLL    driver extension (DirectDraw/Direct3D HAL)
        ELSAVEAV.VXD    virtual mini display driver VICTORY Erazor
        ELSAVEAI.INF    device information file for VICTORY Erazor
        ELSAVEAA.DLL    driver extension
        ELSAVEAR.VXD    driver extension
        ELSAVEAS.DLL    driver extension
        VGARTD.VXD      AGP-support for Windows 95 OSR-2.1
        ELSAVE3D.DLL    "ELSA 3D Settings" utility
        ELSAVE3D.INF    "ELSA 3D Settings" utility setupfile
        ELSAVEA2.VXD    VxD for Multimonitor-Support (only Win98)
        ELSAVEAO.DLL    OpenGL-ICD file
        ELSA3D_DE.DLL   Language extension for "ELSA 3D Settings"
        EVE3D_FR.DLL    Language extension for "ELSA 3D Settings"
        ELSAVE3D.HLP	Helpfile for "ELSA 3D Settings"
        EVE3D_DE.HLP    Helpfile for "ELSA 3D Settings" 
        EVE3D_FR.HLP    Helpfile for "ELSA 3D Settings"  
        WINMAN.EXE      "ELSA Settings" utility 
        WINMAN.DLL      "ELSA Settings" extension
        WINMAN.INF      "ELSA Settings" information file
        WINMAN.MON      "ELSA Settings" extension
        WINMAN-J.HLP    "ELSA Settings" helpfile
        WINMAN-F.HLP    "ELSA Settings" helpfile
        WINMAN-E.HLP    "ELSA Settings" helpfile  
        WINMAN-D.HLP    "ELSA Settings" helpfile  
        WINMAN-J.CNT    "ELSA Settings" extension
        WINMAN-F.CNT    "ELSA Settings" extension 
        WINMAN-E.CNT    "ELSA Settings" extension 
        WINMAN-D.CNT    "ELSA Settings" extension 

        In case of trouble during or after installation, please make
        sure you have all the files mentioned above!


------------------------------------------------------------------------

3.      Installation

      
3.1     First installation of ELSA Display Driver

        First install Windows 95/98 without special drivers for the 
        ELSA graphics board. The installation procedure should
        find a PCI VGA-compatible display adapter and ask for a
        "Driver from disk provided by hardware manufacturer".
        - Push the "OK"-button
        - "Copy manufacturer's files from:"
          CD-Drive: this directory (e.g.: E:\VICTORY\ERAZOR\WIN95)
          The neccessary files will be copy and Windows 95/98 asks 
          for restart.
        - Push the "Yes" or OK button to restart


        Normally you need to boot your system. Push the button "Restart
        now".

3.2     Manuell installation of ELSA Display Driver

        - Start the dialog "Properties for Display" by clicking right
          mouse button on the desktop or per Control Panel.
        - Select the Property Page "Settings"
        - Push the button "Change Display Type...". A dialog "Change
          Display Type" will pop up.
        - Push the button "Change..." inside the frame "Adapter Type".
          You will see the "Select Device" dialog.
        - In this dialog push the button "Have Disk..." and change to
          the WIN95 directory on the ELSAware CD for your WINNER board.
        - Select in the "Manufacturer" list ELSA WINNER Display Driver
          and in the list "Models" your WINNER board.
        - If you use an ELSA monitor, make the same procedure for
          "Monitor Type" in the "Change Display Type" dialog.
        - Close the dialog "Change Display Type". At this time the
          screen flickers a moment. This is not a bug! Windows tries to
          find out, which graphics modes are available with this
          driver.
        - Now you can select resolution and color depth in the main
          dialog "Properties for Display". For the first installation
          you should select 1024x768 and 256 colors. This configuration
          is available for all memory configurations on all ELSA
          Boards.
        - Close "Properties for Display" by "OK" or "Apply
          now".

        After the restart the configuration of the ELSA display adapter
        Driver starts from the Windows desktop.

          - Start the dialog "Properties for Display" by clicking right
            mouse button on the desktop or per Control Panel.
          - Select the Property Page "Settings" or "ELSA WINman".
          - Property Page Settings:
            Standard-Windows-Dialog for changing resolution, color
            depth and font size.
          - Property Page ELSA WINman
            ELSA WINman gives you full control to configure your ELSA
            display adapter perfectly. You can change resolution, color
            depth and refresh rate, screen position etc.

        Normally you need to boot your system. Push the button "Restart
        now".

        In all following Windows sessions you can change the resolution
        without rebooting your system.


------------------------------------------------------------------------

4.      Revision History

        This section describes changes to the previous releases of this
        disk.

        Version 4.10.01.0177
        - first released version

        Version 4.10.01.0201
        - some minor bugfixes

        Version 4.10.01.0202
        - some minor bugfixes
      
        Version 4.10.01.0210
        - some minor bugfixes
        - better TV out performance

        Version 4.10.01.0300
        - better performance and output quality
        - Integration of OpenGL support
        - Feature "ELSA 3D Settings" integrated

        Version 4.10.01.0302
        - fixed an optical bug with follow up menues
        - Anti-Aliasing will only work with graphic adapters with 
          more than 6 MB RAM on it.            
        - fixed optical colorbugs on modes with 256 colors
          
        Version 4.10.01.0303
        - fullscreen on PAL TV out implemented
        - "More 3D" in "3D Settings" bug fixed for Windows 95
------------------------------------------------------------------------

5.      Release notes

5.1     DirectDraw/Direct3D support

        The display driver do support DirectDraw/Direct3D from DirectX 5,
        but to use it in an application, you must install DirectDraw/
        Direct3D. The Microsoft DirectDraw/Direct3D components are not
        included in the standard retail version of Windows 95. You need
        an installation of DirectX 5.

        To install DirectDraw/Direct3D use the CDSETUP from your
        WINNERware CD or start the DXSETUP.EXE in the folder:
        Drive:\ELSAWARE\DDRAW\DIRECTX  
        
5.2     AGP and Windows 95

        AGP is supported only by the Windows version OSR-2.1. This is
        available after upgrading a Windows 95b (OSR2) version by the
        USB-Update 'USBSUPP.EXE'.
        The version number of your installed Windows can be found in
        the registry under: HKEY_LOCAL_MACHINE\SOFTWARE\Microsoft\
        Windows\CurrentVersion\Version and VersionNumber.
        The Entries for OSR-2.1 are:

        Version       "Windows95"
        VersionNumber "4.03.1212" or "4.03.1214"


------------------------------------------------------------------------

6.      Known Bugs and Operating Notes

        This section documents known anomalies or problems and gives
        hints on work arounds.

6.1     Version 4.10.01.0302 or higher

6.1.1   Installation over an existing nVIDIA-driver

        If you install the ELSA Display Driver over an nVIDIA Display Driver,
        the key HKLM\Software\Microsoft\Windows\CurrentVersion\
        OpenGLDrivers\RIVA128 will not actualised. Replace "nv3ogl.dll" with
        "elsaveao.dll"

6.1.2   "OpenGL"

        The hardware support for OpenGL only works only at 16 bpp colordepth 
        up to screenmode 800x600 Pixel.

        OpenGL based screensavers, e.g. 3D Pipes, may occur some 
        malfunctions on some systems if powermangement is activated. 


6.1.3   "G-Police" on TV

        If the game "G-Police", - possibly other applications too,
        has blit errors, you have to disable the Direct3D
        Anti-Aliasing-Support in the "ELSA D3D-Settings".
        (Only with graphics hardware with less than 6 MB RAM)  

6.1.4   "Quickres" change on TV

        If you change the colordepth with "Quickres" on TV-Out and after that
        restarts in DOS-Mode, the screen remains black. So please always
        reboot your PC after changing the screenmode.
        

6.1.5   There may occur misrepresentation of colors and displays by viewing
        MPEG files with "ELSA Motion" extension boards.


------------------------------------------------------------------------
